

HW group s.r.o. FOR RELEASE: IMMEDIATELY

Rumunská 26

Praha, 120 00

<http://www.HW-group.com>

Contact: Jan Rehak,


E- mail: [Rehak@HWg.cz](mailto:Rehak@HWg.cz)

Tel.: +420 222 511 918

Prague, 13th April 2010

**IP WatchDog HWg-WR02a: Ping Restarter**

*IP WatchDog WR02a monitors whether a controlled device, or an Internet connection, is “alive”. If the correct reply is not received in time, the controlled device is restarted using a relay, or a back-up connection is activated.*

**

HW group extends the portfolio of IP WatchDog products and introduces an industrial version of IP WatchDog HWg-WR02a – “ping restarter”. This term describes a product designed for monitoring the functionality of another device over IP (PING/WEB) or serial line (RS-232).

IP WatchDog can monitor two devices (two independent channels, two 110/230VAC relays). Industrial applications can benefit from DIN rail mount.

Failures are detected with five distinct methods, separately for each channel (Ping Tx/Rx, Web page request/push, RS-232 data).

* **Operation monitoring / IP restart**

Servers / routers; IP video cameras; WiFi links / access points; industrial systems

* **Connectivity monitoring**   
  Activation of a back-up link; detection of connectivity outage (relay >> horn); monitoring of ADSL and cable modems; security and access control systems

**About HW group**

* HW group s.r.o. is based in the Czech Republic. Since 2000, HW group develops and distributes network technology products, including networked sensors. The product portfolio is targeted to networked measuring and control. Approximately 10% of the production is sold in the Czech Republic, 60% is destined to the EU markets, and 30% is exported outside of the European Union.

# # #